**On / Off Board Check List Joan III**

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| **Date** |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |
| **On Board** |  |  |  |  |  |  |  |
| Open Sea cocks engine, head and **close cooling**; log install fully |  |  |  |  |  |  |  |
| Safety Scavenger Hunt or Safety Check List |  |  |  |  |  |  |  |
| Electrical Cable disconnect after switching off |  |  |  |  |  |  |  |
| Oil, cooling water, bilge under engine clean/dry |  |  |  |  |  |  |  |
| **Off Board** |  |  |  |  |  |  |  |
| Close 3 sea cocks head, engine and fridge (2); key engine inside |  |  |  |  |  |  |  |
| Close hatches tight |  |  |  |  |  |  |  |
| A/C on de-humidifier (on and then on and low simultaneously) |  |  |  |  |  |  |  |
| LPG off inside, switch and valve |  |  |  |  |  |  |  |
| Check bilge pump |  |  |  |  |  |  |  |
| Other switches off |  |  |  |  |  |  |  |
| Small electronics (VHF, GPS) and documents home |  |  |  |  |  |  |  |
| Protection plates on instruments |  |  |  |  |  |  |  |
| Garbage and cooling empty |  |  |  |  |  |  |  |
| Flags down and stored |  |  |  |  |  |  |  |
| Halyards from masts |  |  |  |  |  |  |  |
| Check dock lines on right mark and fenders |  |  |  |  |  |  |  |
| Electrical feed secured |  |  |  |  |  |  |  |
| Genoa secured or off for long time |  |  |  |  |  |  |  |
| Sail covers secured; halyards, sheets stowed |  |  |  |  |  |  |  |
| Lazarettes locked; Keys Stowed |  |  |  |  |  |  |  |
| Winch Handles stowed |  |  |  |  |  |  |  |
| Dodger covered |  |  |  |  |  |  |  |
| Engine Time |  |  |  |  |  |  |  |
| Gauge Diesel Level |  |  |  |  |  |  |  |
| **Repairs:** |
| Diesel 4/25 31AG (fueled 15), oil ok. |
| Tack pulley for genoa |
| Bulkhead |
|  |
| **Spares** |
| Impeller | Oil Filter STM0051 | Racor Filter 2010 SM OR 2u | Fuel Water Separator STM 3690 | Fuel Pump Filter STM 4050 | V Belt  | Medical Kit |
| 3 new | 1 | 4 | 3 | 1 | 1 unused | unused |