**On / Off Board Check List Joan III**

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Date** | | | | | |  |  |  |  | |  |  |  |
|  | | | | | |  |  |  |  | |  |  |  |
|  | | | | | |  |  |  |  | |  |  |  |
| **On Board** | | | | | |  |  |  |  | |  |  |  |
| Open Sea cocks engine, head and **close cooling**; log install fully | | | | | |  |  |  |  | |  |  |  |
| Safety Scavenger Hunt or Safety Check List | | | | | |  |  |  |  | |  |  |  |
| Electrical Cable disconnect after switching off | | | | | |  |  |  |  | |  |  |  |
| Oil, cooling water, bilge under engine clean/dry | | | | | |  |  |  |  | |  |  |  |
| **Off Board** | | | | | |  |  |  |  | |  |  |  |
| Close 3 sea cocks head, engine and fridge (2); key engine inside | | | | | |  |  |  |  | |  |  |  |
| Close hatches tight | | | | | |  |  |  |  | |  |  |  |
| A/C on de-humidifier (on and then on and low simultaneously) | | | | | |  |  |  |  | |  |  |  |
| LPG off inside, switch and valve | | | | | |  |  |  |  | |  |  |  |
| Check bilge pump | | | | | |  |  |  |  | |  |  |  |
| Other switches off | | | | | |  |  |  |  | |  |  |  |
| Small electronics (VHF, GPS) and documents home | | | | | |  |  |  |  | |  |  |  |
| Protection plates on instruments | | | | | |  |  |  |  | |  |  |  |
| Garbage and cooling empty | | | | | |  |  |  |  | |  |  |  |
| Flags down and stored | | | | | |  |  |  |  | |  |  |  |
| Halyards from masts | | | | | |  |  |  |  | |  |  |  |
| Check dock lines on right mark and fenders | | | | | |  |  |  |  | |  |  |  |
| Electrical feed secured | | | | | |  |  |  |  | |  |  |  |
| Genoa secured or off for long time | | | | | |  |  |  |  | |  |  |  |
| Sail covers secured; halyards, sheets stowed | | | | | |  |  |  |  | |  |  |  |
| Lazarettes locked; Keys Stowed | | | | | |  |  |  |  | |  |  |  |
| Winch Handles stowed | | | | | |  |  |  |  | |  |  |  |
| Dodger covered | | | | | |  |  |  |  | |  |  |  |
| Engine Time | | | | | |  |  |  |  | |  |  |  |
| Gauge Diesel Level | | | | | |  |  |  |  | |  |  |  |
| **Repairs:** | | | | | | | | | | | | | |
| Diesel 4/25 31AG (fueled 15), oil ok. | | | | | | | | | | | | | |
| Tack pulley for genoa | | | | | | | | | | | | | |
| Bulkhead | | | | | | | | | | | | | |
|  | | | | | | | | | | | | | |
| **Spares** | | | | | | | | | | | | | |
| Impeller | Oil Filter STM0051 | Racor Filter 2010 SM OR 2u | Fuel Water Separator STM 3690 | Fuel Pump Filter STM 4050 | V Belt | | | | | Medical Kit | | | |
| 3 new | 1 | 4 | 3 | 1 | 1 unused | | | | | unused | | | |